Material Safety Data Sheet
SECTION I - COMPANY IDENTIFICATION
PRODUCT: EMKARATE RL 32S						CAT. NO.:	LE32SQ, LE32S1, LE32S5, LE32S55
PACKED & DISTRIBUTED BY:						TELEPHONE NUMBERS:
Virginia KMP Corporation							Office:		1-(214) 330-7731
4100 Platinum Way								Emergency Only:	1-(800) 424-9300
Dallas, Texas 75237
SECTION II - HAZARDOUS INGREDIENTS
OSHA Hazardous Components (29 CFR 1910.1200)				EXPOSURE LIMITS: 8 HR. TWA
									OSHA PEL		ACGIH TLV
Polyol ester with antioxidant*							NE			NE
*   Ingredients not precisely identified are proprietary or nonhazardous.

SECTION III - HAZARDS IDENTIFICATIONS
EMERGENCY OVERVIEW:	WARNING!  Harmful if swallowed.  Skin and eye irritant.
POTENTIAL HEALTH EFFECTS:
	INHALATION:	No toxic effects are expected.  High concentrations of mist may be irritating to upper respiratory tract.
	EYE CONTACT:	May cause irritation following contact.
	SKIN CONTACT:	Repeated or prolonged contact may cause mild irritation.  May aggravate pre-existing skin disorders.
	INGESTION:	This material is slightly toxic.  Irritation of gastrointestinal tract may develop following ingestion.
	CHRONIC Effects:	None known
	NOTE:
	CARCINOGENICITY: LISTED IN NTP?   No			IARC?   No			OSHA Regulated?   No

SECTION IV - FIRST AID MEASURES
INHALATION:	Remove victim to fresh air.  If a cough or other respiratory symptoms develop, consult a physician.
EYE CONTACT:	Immediately flush with plenty of water for 15 minutes.  If redness, itching, or a burning sensation develops, get medical attention.
SKIN CONTACT:	Wash material off of skin with plenty of soap and water.  If redness, itching, or burning sensation develops get medical attention.  Wash clothes before reuse.
INGESTION:	DO NOT INDUCE VOMITING.  Give 1 or 2 glasses of water to drink.  If gastrointestinal symptoms develop, consult a physician.

SECTION V - FIRE FIGHTING MEASURES
FLASHPOINT (TEST METHOD):	392 F,   200 C   (PMCC)
FLAMMABLE LIMITS:		LOWER:   NAP				UPPER:   NAP
AUTOIGNITION TEMPERATURE:	ND
GENERAL HAZARD:
FIRE FIGHTING INSTRUCTIONS:	Approach fire from upwind side.  Avoid breathing smoke, fumes, mist or vapors on downwind side.  Firefighters wear protective clothing and self contained breathing apparatus.
EXTINGUISHING MEDIA:	Water fog, foam, carbon dioxide, dry chemical, halogenated agents.
HAZARDOUS COMBUSTION PRODUCTS:	Smoke and fumes, carbon monoxide, carbon dioxide.

SECTION VI - ACCIDENTAL RELEASE MEASURES
LAND SPILL:	Wear skin and respiratory (if mist or vapors are present) protection during cleanup.  Contain spill.  Keep out of sewers and drains.  Soak up material with absorbent and shovel into a chemical waste container.
WATER SPILL:	Notify proper authorities.
Clean up leaks/spills immediately to prevent soil or water contamination.

SECTION VII - HANDLING AND STORAGE
HANDLING:	Product is highly hydroscopic.  Keep container closed tightly.
STORAGE:	Follow normal storage practices.  No special storage requirements necessary.

SECTION VIII - EXPOSURE CONTROLS/PERSONAL PROTECTION
ENGINEERING CONTROLS:	Local exhaust ventilation is recommended.
PERSONAL PROTECTION:	Use chemical impervious gloves and apron, chemical goggles or full face shield.  Respiratory protection is not normally needed under proper conditions of use and storage.  Use MSHA - NIOSH approved respirator for organic vapors, dust and mists whose TLV is greater than 0.05 mg/m3.

SECTION IX - PHYSICAL AND CHEMICAL PROPERTIES
VAPOR PRESSURE @ 20 C: <10					VAPOR DENSITY (Air=1): NA
SPECIFIC GRAVITY (H2O=1): 0.9725					EVAPORATION RATE (H2O=1): NAP
SOLUBILITY IN WATER: Nil						VOC (LB/GAL): NAP
pH: NAP								FREEZING POINT: NA
BOILING POINT: 482 F, 250 C
APPEARANCE & ODOR: Pale straw color with mild odor.

SECTION X - STABILITY AND REACTIVITY
STABILITY:	Stable.
CONDITIONS TO AVOID:	None known.
MATERIALS TO AVOID:	Oxidizing agents.
HAZARDOUS DECOMPOSITION PRODUCTS:	From combustion: smoke, carbon monoxide, carbon dioxide.
HAZARDOUS POLYMERIZATION:	Will not occur.

SECTION XI - TOXICOLOGICAL INFORMATION
From preparation similar to polyol ester with antioxidant	LD50:	>2000 mg/kg	(oral - rat)

SECTION XII - ECOLOGICAL INFORMATION
No data

SECTION XIII - DISPOSAL CONSIDERATIONS
Discarded product is not a hazardous waste under RCRA, 40 CFR 261.

SECTION XIV - TRANSPORTATION INFORMATION
PROPER SHIPPING NAME:	Not regulated material, liquid				
HAZARD CLASS:		NA					
IDENTIFICATION NUMBER:	NA
DOT Emergency Guide #:	NA
Reportable Quantity (RQ):	NA
International:		NA

SECTION XV - REGULATORY INFORMATION
TSCA (Toxic Substance Control Act):	Components of this product are listed on the TSCA Inventory.
CERCLA (Comprehensive Environmental Response, Compensation and Liability Act):	Not listed.
SARA TITLE III (Superfund Amendments and Reauthorization Act):	Not listed.
CALIFORNIA PROPOSITION 65:	Not listed.

SECTION XVI - OTHER INFORMATION
State Right-to-Know Programs:	Not listed.
NFPA Ratings
	Health:		1
	Flammability:	1
	Reactivity:	0
	HMIS Protective Equipment:	X   See your supervisor
Revised: 10/2001